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Rolling Stock Checklist – Must be carried out a minimum of every 12 months


	COACH DESCRIPTION/NAME 
	


TWO COMPETENT PERSONS  TO CARRY OUT INSPECTION
	Name: 
	
	
	Date: 
	

	Name: 
	
	
	 
	


BOGIES
	|_| No damage to wheel treads.
|_| Assessment of wheel wear -  Coning, flange depth and radius 
|_| Wheels are secure on axles – gaps, lateral movement etc. Back to back should be around 172mm.
|_| Check bearings are tight on axles – no lateral movement.
|_| Wheels turn freely.
|_| All springs are present and correctly located.
|_| No excessive movement between axle boxes and keeps (independent sprung axles).
|_| Full travel of axle boxes in keep or suspension – one person watches while other person brings    weight to bear on the coach to check the travel.
|_| All bolts in place and not loose (spanner only required to check if any bolts are found to be loose).
|_| Bogie swivel – check bogies can rotate freely.
|_| Bogie Pivot – Tight enough to restrict tilting but not too tight to restrict rotation. 
|_| Oil/grease to axle boxes and keeps.
BODY WORK
	|_| Check no snags, flaking paint or sharp points that can cause injury.
|_| Structurally sound.
|_| Seats are secure and do not move (Mardyke Coaches).
|_| Bogie cross plates are tight
|_| Couplings are secure and in good condition


BRAKES
	|_| Vacuum system will pressurise and hold at 16” hg.
|_| Brakes work sufficiently to lock or nearly lock wheels when coach unloaded state.
|_| Visually inspect hoses for abrasions and wear.
NOTES
	COACH IS FIT/NOT FIT (delete as appropriate) FOR PUBLIC RUNNING
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